Modbus TCP DAServer

Wonderware Modbus TCP (MBTCP) DAServer 1.1 (1.1.0)

Overview

> The Wonderware® MBTCP DAServer (referred to as the DAServer throughout the remainder of this user’s guide) is a Microsoft® Windows® application program that acts as a communications protocol server. It allows other Windows application programs access to data in the (Schneider’s) Modicon family of controllers (also referred to as devices), including the TSX Quantum and TSX Momentum that are connected to the DAServer through the computers’ Ethernet ports and the Modbus TCP/IP protocol. The MBTCP DAServer also provides connectivity to the Modicon Micro, Compact 984, and TSX Momentum controllers through a Modbus Bridge (174 CEV 300 10). While the DAServer is primarily intended for use with Wonderware InTouch® (Version 7.11 Patch 02 and later), it may be used by any Microsoft Windows program capable of acting as a DDE, SuiteLink™, or OPC client that can also coexist with FactorySuite™ 2000 and greater.

# Readme

For the product readme file, click here: DASMBTCP ReadMe

# User’s Guide

For the product user's guide, click here: DASMBTCP User's Guide

# Product Installation Guide

For the product installation guide, click here: DASMBTCP Installation Guide. This guide provides the instruction when the installation of the product is started.

# Installing the Product

To install the product directly from this CD, click here: DASMBTCP. You must choose the Open option to launch the product installation program. Follow the instructions on your screen to complete the installation.

If you want to archive the product installation to disk, click here: DASMBTCP directory. The Windows Explorer window will be posted. Copy all files and directories in that location to the appropriate directory on your disk.

# Device Integration Objects (DIObjects)

If you are running in an ArchestrA environment, DIObjects for DASMBTCP is available. Please click: DASMBTCP DIObjects.