ReadMe Demo

# Wonderware SCADAlarm 6.0 SP2 Software Demo ReadMe

Last revision: 3/29/2007

This document contains important information about WonderwareÒ SCADAlarmÔ 6.0 SP2 Demo version, the SCADAlarm demo application, and the InTouchÒ demo application.

SCADAlarm Demo Version

SCADAlarm and InTouch Demo Applications

# SCADAlarm Demo Version

The SCADAlarm 6.0 SP2 Demo version is designed to familiarize you with the SCADAlarm software and its applications. To that end, the complete SCADAlarm version 6.0 SP2 package is provided, with only one difference: the physical modem driver has been replaced by a simulated telephone and pager. The operation of this SCADAlarm 6.0 SP2 Demo version is therefore identical to the real thing, except the inconvenience of physical phones and lines and pagers has been removed.

However, when you decide to install an actual working SCADAlarm system, all you'll need is the modem and license file. ALL OF YOUR WORK WILL STILL BE FUNCTIONAL!

In addition to the usual SCADAlarm menu window, two windows are displayed: one that looks like a telephone, and one that looks like a pager. These are designed to operate roughly like their real-life counterparts, but the characteristics of actual telephone systems are not completely duplicated. There is no busy signal, there are no modem negotiation delays, and so forth.

If you have installed the Demo version and want to switch to the Full version, simply run the SCADAlarm setup program and choose to modify your installation. The SCADAlarm setup program will switch your installation from the Demo version to the Full version. Any changes you made in the Demo version will be retained when you switch to the Full version.

If you have installed the Full version and want to switch to the Demo version, run the SCADAlarm setup program and choose to modify your installation. The SCADAlarm setup program will switch your installation from the Full version to the Demo version. Any changes you made in the Full version will be retained when you switch to the Demo version. You can later switch back to the Full version.

## System Requirements

The SCADAlarm 6.0 SP2 Demo version requires a SCADAlarm-compatible system. A Windows sound system capable of recording and playing back is needed. This sound system will be in use throughout the entire SCADAlarm Demo session. If a sound device is not available, the simulated phone and pager will not appear.

If a Wonderware SCADAlarm license file is found, this demonstration will run continuously; otherwise, it will time out in two hours.

The supplied sound files are assembled from a variety of sources and have been filtered to increase intelligibility over telephone lines; therefore, they may not sound as crisp as a CD.

NOTE: Be sure your microphone and Wave devices are enabled and their volume is turned up in your Mixer panel.

## Operating Instructions

### General

You can move the phone or pager windows by clicking and dragging on the top or bottom plastic areas. Right-click on the phone or the pager for a menu. Most of the options are self-explanatory.

### Pagers

The three buttons on the top of the telephone mimic the three buttons on the top of the pager. The arrows scroll forward and backward in the pager message queue. The Dot button selects the most-recent page. The pager stores fourteen pages; after that the least recent is discarded on receipt of a new page. Hovering over the pager or phone LCD display shows the complete list of stored pages.

### Telephone

The telephone can be set to respond to one pager ID. If an operator is being paged and the ID matches that of the telephone, it'll show up on the telephone; the pager gets all the rest.

### Incoming or Outgoing Call

To place a call to the SCADAlarm software, or to answer a call from the SCADAlarm software, click on the TALK key on the telephone. On a call from the SCADAlarm software, the telephone's LCD display shows which number was dialed.

### Making Recordings

Within the SCADAlarm software, there are many opportunities to record files. When the record window pops up, this Demo will record a WAV file for use by the demo and for the SCADAlarm menu system. Also, you can record using your favorite sound editor and use those for your sound files. Just drop them into the VoxFiles directory under your SCADAlarm installed directory, and this demo will locate them. If you copy files in while SCADAlarm 6.0 SP2 Demo is running, you can choose to import the files using the phone's menu. If you copy in the files before the SCADAlarm software starts up, they will be detected.

If you use another sound file editor (such as Windows Sound Recorder), remember that SCADAlarm 6.0 SP2 Demo requires 8 MHz, 16-bit, mono PCM sound files with a .WAV extension; this is well within the capabilities of any sound system.

This demo is intended for use with full-duplex sound hardware. If that's not the case, you will be informed that recording will not work. However, playback (which is 99% of this demo) will work fine.

< top of document >

# SCADAlarm and InTouch Demo Applications

Two demo applications are included: a SCADAlarm "tank" demo application and an InTouch "tank" demo application. The SCADAlarm application is located in the \SCADAlarm Applications folder of the SCADAlarm CD. The InTouch application is located in the \InTouch Applications folder of the SCADAlarm CD. You will need the InTouch 9.0 software or later to run the InTouch demo application.

The SCADAlarm demo is pre-configured with two default administrators:

· 001 R. Kestra

· 002 A. G. Bell

There are also two default users:

· 003 Klaatu

· 004 W. Rancher

The PIN for all administrators and users is 0000. These operators will be notified on the virtual pager and phone when the demo application is running.

You can use the two applications together to explore the features of the SCADAlarm software. The InTouch demo application is of a city water system. The application includes tags that have corresponding alarm tags in the SCADAlarm tank demo application. You can turn a switch in the InTouch application in WindowViewer to start the simulation of the water system. For example, when the water tank level reaches the low limit, an alarm will be triggered. Also, you can click the Remote Pump Station graphic in the InTouch application to manually trigger an intrusion alarm. The alarms will be triggered in the SCADAlarm software, and the SCADAlarm software will call the virtual phone or pager.

< top of document >

### © 2007 Invensys Systems, Inc. All Rights Reserved.