<?xml version="1.0" encoding="UTF-8"?>
<CONFIGURATIONRULES NAME="FSGateway" PACKAGEHOSTID="{7F5B8DEE-AB78-11D4-93E4-00B0D0201D61}" EDITORHOSTID="{5C9AF1AA-AEC8-11D4-93E6-00B0D0201D61}">
   <HIERARCHYNODE TYPE="$ROOT$">
      <CHILDRULES ENABLEGLOBALPARAMETERS="1">
         <SuiteLink MAXOCCURRENCES="1000000"/>
         <DDE MAXOCCURRENCES="1000000"/>
         <ArchestrA MAXOCCURRENCES="1"/>
         <OPC MAXOCCURRENCES="1000000"/>
         <InTouch MAXOCCURRENCES="1000000"/>
      </CHILDRULES>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <UpdateInterval>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>1000</DEFAULTVALUE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>100000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Device Group Update Interval</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Update interval of default topics for hierarchies without overriding configuration</PROPERTYEDITHELP>
         </UpdateInterval>
         <SlowPollInterval>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>10000</DEFAULTVALUE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>100000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Slow Poll Interval</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Update interval of topics for hierarchies in slow poll mode</PROPERTYEDITHELP>
         </SlowPollInterval>
         <CaseSensitive>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Case Sensitive</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>T/F</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>TRUE means case-sensitive Device Group and Item ID names</PROPERTYEDITHELP>
         </CaseSensitive>
         <DefaultPokeMode>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>2</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>2</PROPERTYMAX>
            <PROPERTYEDITHEADER>Poke Mode</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>0=Control, 1=Transition, 2=Optimized</PROPERTYEDITHELP>
         </DefaultPokeMode>
         <DefaultDelimiter>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>.</DEFAULTVALUE>
            <PROPERTYEDITHEADER>Delimiter</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Delimiter for hierarchies not configured</PROPERTYEDITHELP>
         </DefaultDelimiter>
         <SimulationMode>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Simulation Mode</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>T/F</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>TRUE means simulate for DAServers that support simulation</PROPERTYEDITHELP>
         </SimulationMode>
         <EnableSystemItems>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>1</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>System Items</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>T/F</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>TRUE to allow system items</PROPERTYEDITHELP>
         </EnableSystemItems>
         <LinkTopicCache>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Device Group Cache</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>T/F</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>TRUE merges all subscription items in a single cache</PROPERTYEDITHELP>
         </LinkTopicCache>
         <UniqueDeviceGroup>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <DEFAULTVALUE>1</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Unique Device Groups</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>T/F</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>TRUE requires all device group names be unique</PROPERTYEDITHELP>
         </UniqueDeviceGroup>
         <ProtocolTimerTick>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <DEFAULTVALUE>50</DEFAULTVALUE>
            <PROPERTYMIN>10</PROPERTYMIN>
            <PROPERTYMAX>100000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Protocol Timer</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Protocol timer tick interval in milliseconds</PROPERTYEDITHELP>
         </ProtocolTimerTick>
         <TransactionTimeout>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <DEFAULTVALUE>60000</DEFAULTVALUE>
            <PROPERTYMIN>10</PROPERTYMIN>
            <PROPERTYMAX>120000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Transaction Timeout</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Default transaction timeout for hierarchies with no configuration</PROPERTYEDITHELP>
         </TransactionTimeout>
         <SubscriptionTransactionRatio>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <DEFAULTVALUE>2</DEFAULTVALUE>
            <PROPERTYACCESSRIGHTS>2</PROPERTYACCESSRIGHTS>
            <PROPERTYMIN>1</PROPERTYMIN>
            <PROPERTYMAX>1000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Transaction to Subscription Ratio</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Subscription / Transaction ratio</PROPERTYEDITHELP>
         </SubscriptionTransactionRatio>
         <TransactionsBacklog>
            <PROPERTYTYPE>VT_UI4</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>50</PROPERTYMAX>
            <PROPERTYEDITHEADER>Diagnostic Backlog Size</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Transactions</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Number of completed transactions kept in diagnostic viewer</PROPERTYEDITHELP>
         </TransactionsBacklog>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="SuiteLink" EDITORID="{C5CEB523-47F4-4E68-0082-60D69852D028}" DELIMITER="." PACKAGEID="{D9A98954-A87D-46F9-BE4B-CC2CBEAD5C8E}">
      <CHILDRULES>
         <Topic MAXOCCURRENCES="100"/>
      </CHILDRULES>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>4</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ServerName>
            <!--Legacy IO Server -->
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>MyServer</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>255</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Adapter IP Host Name or Address</PROPERTYEDITHELP>
         </ServerName>
         <ServerNode>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>localhost</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Node</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Server Node</PROPERTYEDITHELP>
         </ServerNode>
         <RestartPeriod>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>30000</DEFAULTVALUE>
            <PROPERTYMIN>10000</PROPERTYMIN>
            <PROPERTYMAX>300000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Period</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Period in ms between between restart attempts.  </PROPERTYEDITHELP>
         </RestartPeriod>
         <RestartAttempts>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>-1</PROPERTYMIN>
            <PROPERTYMAX>1000000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Attempts</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>RestartAttempts</PROPERTYEDITHELP>
         </RestartAttempts>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="DDE" EDITORID="{B50A8A33-E808-4880-008C-F40E4DD4D2AF}" DELIMITER="." PACKAGEID="{D9A98954-A87D-46F9-BE4B-CC2CBEAD5C8E}">
      <CHILDRULES>
         <Topic MAXOCCURRENCES="100"/>
      </CHILDRULES>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>4</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ServerName>
            <!--Legacy IO Server -->
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>MyServer</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>255</PROPERTYMAX>
            <PROPERTYEDITHEADER>Host Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Adapter IP Host Name or Address</PROPERTYEDITHELP>
         </ServerName>
         <ServerNode>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>localhost</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Node</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Server Node</PROPERTYEDITHELP>
         </ServerNode>
         <RestartPeriod>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>30000</DEFAULTVALUE>
            <PROPERTYMIN>10000</PROPERTYMIN>
            <PROPERTYMAX>300000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Period</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Period in ms between between restart attempts.  </PROPERTYEDITHELP>
         </RestartPeriod>
         <RestartAttempts>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>-1</PROPERTYMIN>
            <PROPERTYMAX>1000000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Attempts</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>RestartAttempts</PROPERTYEDITHELP>
         </RestartAttempts>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="ArchestrA" EDITORID="{F05B061B-060E-4085-00B0-2301D1CF88B0}" PACKAGEID="{D9A98954-A87D-46F9-BE4B-CC2CBEAD5C8E}" DELIMITER=".">
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>ReadOnly</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>ReadOnly</PROPERTYEDITHELP>
         </ReadOnly>
         <UserName>
            <!--User Name-->
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE/>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>64</PROPERTYMAX>
            <PROPERTYEDITHEADER>User Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>User Name</PROPERTYEDITHELP>
         </UserName>
         <Password>
            <!--Password-->
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>8BCBD712F0DEC50500B75D6796923E7F2AC80888FB7B3760094C6D8D080BB739FD669D2EE6617F8A</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Password</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Password</PROPERTYEDITHELP>
         </Password>
         <RestartPeriod>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>30000</DEFAULTVALUE>
            <PROPERTYMIN>10000</PROPERTYMIN>
            <PROPERTYMAX>300000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Period</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Period in ms between between restart attempts.  </PROPERTYEDITHELP>
         </RestartPeriod>
         <RestartAttempts>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1000000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Attempts</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>RestartAttempts</PROPERTYEDITHELP>
         </RestartAttempts>
      </PROPERTYRULES>
      <CHILDRULES ENABLEDEVICEITEMS="1" ENABLEDEVICEGROUPS="0">
         <ArchestrAGroup MAXOCCURRENCES="100"/>
      </CHILDRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="OPC" EDITORID="{DF99C653-3105-486B-0090-A30A56E50064}" DELIMITER="." PACKAGEID="{D9A98954-A87D-46F9-BE4B-CC2CBEAD5C8E}">
      <CHILDRULES>
         <OPCGroup MAXOCCURRENCES="100"/>
      </CHILDRULES>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>4</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ServerName>
            <!--OPC Server-->
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE/>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>255</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Server Name</PROPERTYEDITHELP>
         </ServerName>
         <ServerNode>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>localhost</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Node</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Server Node</PROPERTYEDITHELP>
         </ServerNode>
         <RunOutOfProc>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>-1</DEFAULTVALUE>
            <PROPERTYMIN>-1</PROPERTYMIN>
            <PROPERTYMAX>0</PROPERTYMAX>
            <PROPERTYEDITHEADER>CoCreate using CLSCTX_LOCAL_SERVER</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>0,-1</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>CoCreate using CLSCTX_LOCAL_SERVER</PROPERTYEDITHELP>
         </RunOutOfProc>
         <RestartPeriod>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>30000</DEFAULTVALUE>
            <PROPERTYMIN>10000</PROPERTYMIN>
            <PROPERTYMAX>300000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Period</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Period in ms between between restart attempts.  </PROPERTYEDITHELP>
         </RestartPeriod>
         <RestartAttempts>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>-1</PROPERTYMIN>
            <PROPERTYMAX>1000000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Attempts</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>RestartAttempts</PROPERTYEDITHELP>
         </RestartAttempts>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="Topic" EDITORID="{8909CE70-6E87-4DC9-00A0-13FB77C17DC1}" DELIMITER=".">
      <CHILDRULES ENABLEDEVICEITEMS="1"/>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Read Only</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>boolean</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Topic is read-only when checked</PROPERTYEDITHELP>
         </ReadOnly>
         <ChangeTopicName>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Change Topic Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>boolean</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Change Topic Name</PROPERTYEDITHELP>
         </ChangeTopicName>
         <TopicName>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>&lt;unknown&gt;</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Topic Name</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Topic Name</PROPERTYEDITHELP>
         </TopicName>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="OPCGroup" DELIMITER="." EDITORID="{4DC1C693-0AF2-436F-008E-6533774C139C}">
      <CHILDRULES ENABLEDEVICEITEMS="1" ENABLEDEVICEGROUPS="0"/>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <UpdateRate>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>1000</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>10000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Update Rate</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>milliseconds </PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Update Rate</PROPERTYEDITHELP>
         </UpdateRate>
         <UseGroupNameAsAccessPath>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Use Group Name as Access Path</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Use Group Name as Access Path</PROPERTYEDITHELP>
         </UseGroupNameAsAccessPath>
         <FullyQualifiedOPCItemPath>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE/>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>FullyQualifiedOPCItemPath</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>FullyQualifiedOPCItemPath</PROPERTYEDITHELP>
         </FullyQualifiedOPCItemPath>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>ReadOnly</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>ReadOnly</PROPERTYEDITHELP>
         </ReadOnly>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="InTouch" EDITORID="{7D4FF362-DEC5-478E-00B1-642A2F64A911}" DELIMITER="." PACKAGEID="{D9A98954-A87D-46F9-BE4B-CC2CBEAD5C8E}">
      <CHILDRULES ENABLEDEVICEITEMS="1">
         <InTouchGroup MAXOCCURRENCES="100"/>
      </CHILDRULES>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>4</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ServerNode>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>localhost</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Node</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Servr Node</PROPERTYEDITHELP>
         </ServerNode>
         <ApplicationPath>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE/>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Application Path</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Application Path</PROPERTYEDITHELP>
         </ApplicationPath>
         <ProtocolType>
            <PROPERTYTYPE>VT_I2</PROPERTYTYPE>
            <DEFAULTVALUE>2</DEFAULTVALUE>
            <PROPERTYMIN>1</PROPERTYMIN>
            <PROPERTYMAX>2</PROPERTYMAX>
            <PROPERTYEDITHEADER>ProtocolType</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ProtocolType</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>ProtocolType</PROPERTYEDITHELP>
         </ProtocolType>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Read Only</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>boolean</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Topic is read-only when checked</PROPERTYEDITHELP>
         </ReadOnly>
         <RestartPeriod>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>30000</DEFAULTVALUE>
            <PROPERTYMIN>10000</PROPERTYMIN>
            <PROPERTYMAX>300000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Period</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>ms</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Period in ms between between restart attempts.  </PROPERTYEDITHELP>
         </RestartPeriod>
         <RestartAttempts>
            <PROPERTYTYPE>VT_I4</PROPERTYTYPE>
            <DEFAULTVALUE>3</DEFAULTVALUE>
            <PROPERTYMIN>-1</PROPERTYMIN>
            <PROPERTYMAX>1000000</PROPERTYMAX>
            <PROPERTYEDITHEADER>Reconnect Attempts</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>RestartAttempts</PROPERTYEDITHELP>
         </RestartAttempts>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="InTouchGroup" EDITORID="{F76F671C-9D5B-4D27-009C-EE570EE852A5}" DELIMITER=".">
      <CHILDRULES ENABLEDEVICEITEMS="1"/>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <ServerNode>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>&lt;unknown&gt;</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Server Node</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Servr Node</PROPERTYEDITHELP>
         </ServerNode>
         <ApplicationPath>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>&lt;unknown&gt;</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Application Path</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Application Path</PROPERTYEDITHELP>
         </ApplicationPath>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Read Only</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>boolean</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Topic is read-only when checked</PROPERTYEDITHELP>
         </ReadOnly>
      </PROPERTYRULES>
   </HIERARCHYNODE>
   <HIERARCHYNODE TYPE="ArchestrAGroup" EDITORID="{F52F6896-B30B-4E1B-00B8-19B02D8D4DE6}" DELIMITER=".">
      <CHILDRULES ENABLEDEVICEITEMS="1"/>
      <PROPERTYRULES>
         <_ImageId>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>256</PROPERTYMAX>
            <PROPERTYEDITHEADER>Image Id</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>Index</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Image Id</PROPERTYEDITHELP>
         </_ImageId>
         <FullyQualifiedArchestrAItemPath>
            <PROPERTYTYPE>VT_BSTR</PROPERTYTYPE>
            <DEFAULTVALUE/>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>250</PROPERTYMAX>
            <PROPERTYEDITHEADER>Prefix</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT/>
            <PROPERTYEDITHELP>Prefix</PROPERTYEDITHELP>
         </FullyQualifiedArchestrAItemPath>
         <ReadOnly>
            <PROPERTYTYPE>VT_BOOL</PROPERTYTYPE>
            <DEFAULTVALUE>0</DEFAULTVALUE>
            <PROPERTYMIN>0</PROPERTYMIN>
            <PROPERTYMAX>1</PROPERTYMAX>
            <PROPERTYEDITHEADER>Read Only</PROPERTYEDITHEADER>
            <PROPERTYEDITUNIT>boolean</PROPERTYEDITUNIT>
            <PROPERTYEDITHELP>Topic is read-only when checked</PROPERTYEDITHELP>
         </ReadOnly>
      </PROPERTYRULES>
   </HIERARCHYNODE>
</CONFIGURATIONRULES>
