==================================================================

   SCADAlarm Sound File Conversion Utility 
   Version 6.0.0
   Copyright 2004 Invensys Systems, Inc.

   Revised 10/26/2004

   Two files accompany this application:

   * VCONVERT.EXE -- The Sound File Conversion Utility executable file.
   * VConvert Readme.txt -- This readme file.


==================================================================

This utility allows you to convert from the following voxfile formats:

* SCADAlarm Rockwell voxfile
* SCADAlarm 3Com voxfile
* SCADAlarm IS-101 voxfile

to the following formats:

* 16-bit 8kHz Mono PCM .WAV 
* 8-bit 8kHz Mono PCM .WAV
* 8-bit 11kHz Mono PCM .WAV
    
   
NOTE:  Rockwell refers to the modem chipset used by the Hayes, MultiTech, and
       Supra voice modems (among others).


==================================================================

Converting from SCADAlarm Voxfile Formats

==================================================================


To convert voxfiles to .wav files:

1.  Start the SCADAlarm Sound File Conversion Utility.

2.  Verify that the desired path for your voxfiles is displayed in the 
    "Show Sound Files in this folder:" box.  To change
    folders, click on the button labeled "..." and select the desired folder.

3.  By default, the "Exclude System Files" box is checked, meaning that none of 
    the "canned" SCADAlarm files will appear in the file list box.  

4.  Select the source file type (Rockwell, 3Com/USR, IS-101) from the Input File Type
    drop-down list.

5.  Select the destination file type (.wav) from the Output File Type
    drop-down list.

6.  Click Convert.  You will be prompted for final confirmation.  Click OK to proceed.

8.  Converted files will be written to a folder named "vox_conv".  The original
    sound files remain unchanged.

9.  Copy the converted files to your SCADAlarm voxfiles folder.
    


